Vicon RO-XL VN207 | Sovereign Sulphur | 24m

|  |
| --- |
| Tray Test Details |
| Machine | **Vicon RO-XL VN207 (VN2070302347)** | Spread Width | **24m** |
| Product | **Sovereign Sulphur** | Rate Setting | **Setting 29** |
| NSTS Certificate | **321364** | Date Tested | **20/01/2023** |
| Test Conditions |
| Forward Speed | **14 km/h** | Ground Condition | **Grass** |
| Wind Speed | **4 km/h** | Wind Direction | **From behind machine** |
| Product Details - Sovereign Sulphur |
| A picture containing text  Description automatically generated | Batch No. | **23/08/2022 09:23** |
| Product Spread Before Today's Test | **No** |
| Lumping In Bag | **No** |
| Density (kg/L) | **1.11** |
| Product strength (kg/Force) |
| **6.5** | **7** | **6.5** | **6** | **5** | **4.5** | **5.5** | **6.5** | **7.5** | **4.5** |
| Average Strength (kg/Force) | **5.95** |
| Grader Box |
| 0 - 2mm | 2 - 3.3mm | 3.3 - 4.75mm | > 4.75mm |
| **0%** | **5%** | **95%** | **0%** |
| Successful Run |
| Disc/Vane/Type | **285/285/285** | Spread Setting | **P** |
| PTO/Disc Speed | **PTO RPM 525** | Rate Setting | **Setting 29** |
| Tilt | **0** | Headland Setting | **N/A** |
| Spreader Height | **75cm from side of disc** |
| Visible Segregation | **No** | Residue on Discs | **No** |
| Measurable Overlap | **5m** | Coefficient of Variation | **9.34%** |
| **Comments: Final spread pattern successful.** |
| A close-up of a piano  Description automatically generated with low confidence12m 0m 12mCoefficient of Variation measures the accuracy of the spread pattern. For fertilisers a CV of 15% (as recommended in EB13739-2) should be attained in field conditions. <10% Excellent, 10%-15% Good, 15%-20% Poor, >20% Unacceptable.There is no CV Pass/Fail for NSTS requirements. |